**San Joaquin Valley**

**Unified Air Pollution Control District**

# Title V Application - INSIGNIFICANT ACTIVITIES

|  |  |
| --- | --- |
| COMPANY NAME: | FACILITY ID: **-** |
| Check the box next to the exemption category from Rule 2020 which describes any insignificant activity or equipment at your facility not requiring a permit. |
| Exemption Category | Rule 2020 Citation | √ | Exemption Category | Rule 2020 Citation | √ |
| Structure or incinerator assoc. with a structure designed as a dwelling for 4 families or less | 4.1 |  | Containers used to store refined lubricating oils | 6.6.8 |  |
| Locomotives, airplanes, and watercraft used to transport passengers or freight  | 4.4 |  |
| Unvented pressure vessels used exclusively to store liquified gases or assoc with exempt equipment | 6.6.9 or 6.13 |  |
| Natural gas or LPG-fired boilers or other indirect heat transfer units of 5 MMBtu/hr or less | 6.1.1 |  |
| Portable tanks used exclusively to store produced fluids for ≤ six months | 6.6.10 |  |
| Piston-type i.c.engine with maximum continuous rating of 50 braking horsepower (bhp) or less | 6.1.2 |  |
| Mobile transport tanks on delivery vehicles of VOCs | 6.6.11 |  |
| Gas turbine engines with maximum heat input rating of 3 MMBtu/hr or less | 6.1.3 |  | Loading racks used for the transfer of less than 4,000 gal/day of unheated organic material with initial boiling point ≥ 302 F or of fuel oil with specific gravity ≥0.8251 | 6.7.1.1 |  |
| Space heating equipment other than boilers | 6.1.4 |  | Loading racks used for the transfer of asphalt, crude or residual oil stored in exempt tanks, or crude oil with specific gravity ≥ 0.8762 | 6.7.1.2 |  |
| Cooling towers with a circulation rate less than 10,000 gal/min, and that are not used for cooling of process water, or water from barometric jets or condensers++ | 6.2 |  |
| Equipment used exclusively for the transfer of refined lubricating oil  | 6.7.2 |  |
| Use of less than 2 gal/day of graphic arts materials | 6.3 |  |
| Equipment used to apply architectural coatings  | 6.8.1 |  |
| Equipment at retail establishments used to prepare food for human consumption | 6.4.1 |  | Unheated, non-conveyorized cleaning equipment with < 10 ft2 open area; using solvents with initial boiling point ≥ 248 F; and < 25 gal/yr. evaporative losses | 6.9 |  |
| Ovens at bakeries with total daily production less than 1,000 pounds and exempt by sec. 6.1.1 | 6.4.3 |  |
| Brazing, soldering, or welding equipment | 6.10 |  |
| Equipment used exclusively for extruding or compression molding of rubber or plastics, where no plastisizer or blowing agent is used | 6.5 |  |
| Equipment used to compress natural gas  | 6.11 |  |
| Containers used to store clean produced water | 6.6.1 |  | Fugitive emissions sources assoc. with exempt equipment | 6.12 |  |
| Containers ≤100 bbl used to store oil with specific gravity ≥ 0.8762 | 6.6.2 |  | Pits and Ponds as defined in Rule 1020 | 6.15 |  |
| Containers ≤ 100 bbl installed prior to 6/1/89 used to store oil with specific gravity ≥ 0.8762 | 6.6.3 |  | On-site roadmix manufacturing and the application of roadmix as a road base material | 6.17 |  |
| Containers with a capacity ≤ 250 gallons used to store org-anic material where the actual storage temperature <150 F | 6.6.4 |  | Emissions less than 2 lb/day from units not included above | 6.19 |  |
| Containers used to store unheated organic material with an initial boiling point ≥ 302 F | 6.6.5 |  | Venting PUC quality natural gas from for sole purpose of pipeline and compressor repair and or maintenance | 7.2 |  |
| Containers used to store fuel oils or non-air-blown asphalt with specific gravity ≥0.9042 | 6.6.6 |  | Non-structural repairs & maintenance to permitted equipment | 7.3 |  |
| Containers used to store petroleum distillates used as motor fuel with specific gravity ≥ 0.8251 | 6.6.7 |  | Detonation of explosives ≤ 100 lb/day and 1,000 lb/year | 7.4 |  |

 No insignificant activities (Check this box if no equipment in the above categories exist at your facility.)

TVFORM–003

 (Rev. September-2001)